Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Configuring Rate Shaping for a Scheduler Node or Queue
- Configuring Port Shaping

# Rate Shaping and Port Shaping Overview

Rate shaping throttles the rate at which queues transmit packets. Rate shaping is TCP friendly; that is, it buffers packets that are above the rate, rather than dropping them.

Port shaping enables you to shape the aggregate traffic through a port or channel to a rate that is less than the line or port rate. With port shaping, you can configure scheduler nodes at the port level, as shown in Figure 1.

Figure 1: Port Shaping on an Ethernet Module

The per-port shaping feature provides the ability to shape the output of a port.

## Related Documentation

- Configuring Rate Shaping for a Scheduler Node or Queue
- Configuring Port Shaping

#### Published: 2010-09-22

Help
|
My Account
|
Log Out