# tcp resequence-buffers global-maximum

#### Syntax

ip tcp resequence-buffers global-maximum globalMaxValue

no [ ip ] tcp resequence-buffers global-maximum

#### Release Information

Command introduced before JunosE Release 7.1.0.
ip keyword made optional in JunosE Release 7.2.0.

#### Description

Specifies a router-wide maximum number of buffers that resequencing queues can contain. Specifying a value of zero (0) turns off the limit. The no version reverts the global maximum buffer value to its default (1000 buffers).

#### Options

- ip—Optional keyword for use with older scripts
- globalMaxValue—Maximum number of buffers in the range 1–65535

#### Mode

Global Configuration