Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# show l2tp dial-out virtual-router

#### Syntax

show l2tp dial-out virtual-router [ allVirtualRouters ] [ detail ] [ state operState ]
[ filter ]

To display summary information:

show l2tp dial-out virtual-router summary [ allVirtualRouters ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Displays dial-out state machine operational status and statistics within the current virtual router context.

#### Options

- allVirtualRouters—Displays dial-out information across all virtual routers
- detail—Displays configuration, state, and statistics
- operState—One of the following operational states:
  - down
  - inService
  - initFailed
  - initPending
- filter—See Filtering show Commands
- summary—Displays aggregate counts for dial-out state machines in each of the possible operational and administrative states

#### Mode

Privileged Exec

#### Published: 2010-10-19

Help
|
My Account
|
Log Out