# vlan auto-configure agent-circuit-identifier

#### Syntax

[ no ] vlan auto-configure agent-circuit-identifier

#### Release Information

Command introduced in JunosE Release 7.3.0.

#### Description

Configures the router to dynamically create VLAN subinterfaces based on the agent-circuit-id option (suboption 1) of the option 82 field in DHCP messages, or based on the DSL Forum VSA 26-1 (Agent-Circuit-Id) in PPPoE PADR and PADI packets. The no version disables the creation of VLAN subinterfaces based on agent-circuit-identifier information.

#### Mode

Profile Configuration