# Monitoring DHCP External Server Configuration Information

#### Purpose

Display information about the router’s DHCP external server application.

#### Action

To display DHCP external server information:

    host1#show ip dhcp-external configuration
     Dhcp External : Enabled
     Auto-Configure : Enabled
     Server-Sync : Enabled
     Disregard-Giaddr-Next-Hop : Enabled
     Detect-Agent-Circuit-Id : Disabled
     Recreate-Subscriber-Interface : Enabled
     Duplicate-MAC-Address : Enabled

     Servers:
     -----------
     10.1.1.1
     10.2.1.1
     10.3.1.1

#### Meaning

Table 110 lists the show ip dhcp-external configuration command output fields.

Table 110: show ip dhcp-external configuration Output Fields

Field Name | Field Description
--- | ---
Dhcp External | Enabled or disabled
Auto-Configure | Enabled or disabled
Server-Sync | Enabled or disabled
Disregard-Giaddr-Next-hop | Enabled or disabled
Detect-Agent-Circuit-Id | Enabled or disabled
Recreate-Subscriber-Interface | Enabled or disabled
Duplicate-MAC-Address | Enabled or disabled
Servers | DHCP servers whose traffic is monitored by the E Series router

#### Related Documentation

- show ip dhcp-external configuration