Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# ntp broadcast

#### Syntax

[ no ] ntp broadcast [ version number ] [ pollInterval ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables NTP broadcast server on a server interface to transmit NTP broadcast packets periodically. You can enable up to 100 NTP broadcast server interfaces. The no version prevents the interface from sending NTP broadcast packets.

#### Options

- number—Integer in the range 1–4; indicates the version of the NTP software on the NTP broadcast server; default value is 3
- pollInterval—Integer in the range 4–17; specifies the poll interval in seconds (as a power of 2) for broadcasting NTP messages; default value is 6 (64 seconds)

#### Mode

Interface Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out