Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# route-map

#### Syntax

Specifying a route map for DVMRP or RIP:

[ no ] route-map mapTag [ interfaceType interfaceSpecifier ]

Defining a route map:

[ no ] route-map mapTag [ permit | deny ] [ sequence ]

Defining a route map for data MDTs:

route-map routeMapName

no route-map

#### Release Information

Command introduced before JunosE Release 7.1.0.
IP PIM Data MDT Configuration mode added in JunosE Release 8.2.0.

#### Description

Specifies a route map for DVMRP, RIP, or data MDTs, or defines the conditions for applying routing policies to filter or modify routes redistributed into or propagated by a routing protocol. The no version deletes the route map.

#### Options

- mapTag—String of up to 32 alphanumeric characters.
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- mapTag—String of up to 32 alphanumeric characters. The redistribute Router Configuration command uses this string to reference this route map. Multiple route maps may share the same map tag.
- permit—If the match criteria are met for this route map and permit is specified, the route is redistributed as controlled by the set actions.
- deny—If the match criteria are met for the route map and deny is specified, the route is not redistributed, and no further route maps sharing the same map tag are examined.
- sequence—Number, in the range 0–65535, that indicates the position a new route map is to have in the list of route maps already configured with the same map tag. If given with the no version of this command, it specifies the position of the route map that should be deleted.

#### Mode

Address Family Configuration (RIP), Global Configuration, IP PIM Data MDT Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out