Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# traps

#### Syntax

[ no ] traps { all | [ virtIfStateChange | nbrStateChange | virtNbrStateChange |
ifConfigError | virtIfConfigError | ifAuthFailure | virtIfAuthFailure | ifRxBadPkt |
virtIfRxBadPkt | txRetransmit | virtTxRetransmit | originateLsa | maxAgeLsa |
ifStateChange ]* }

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies OSPF trap settings. The no version removes all OSPF trap settings or any specified traps.

#### Options

- all—Enables all OSPF traps
- virtIfStateChange—Sets a trap to indicate a state change on an OSPF virtual interface
- nbrStateChange—Sets a trap to indicate a state change on a nonvirtual OSPF neighbor
- virtNbrStateChange—Sets a trap to indicate a state change on a virtual OSPF neighbor
- ifConfigError—Sets a trap to indicate a configuration mismatch with a nonvirtual neighbor
- virtIfConfigError—Sets a trap to indicate a configuration mismatch with a virtual neighbor
- ifAuthFailure—Sets a trap to indicate an authentication failure on a nonvirtual interface
- virtIfAuthFailure—Sets a trap to indicate an authentication failure on a virtual interface
- ifRxBadPkt—Sets a trap to indicate that a packet has been received that cannot be parsed
- virtIfRxBadPkt—Sets a trap to indicate that a packet has been received on a virtual interface that cannot be parsed
- txRetransmit—Sets a trap to indicate that a packet has been retransmitted on a nonvirtual interface
- virtTxRetransmit—Sets a trap to indicate that a packet has been retransmitted on a virtual interface
- originateLsa—Sets a trap to indicate that a new LSA has been originated by this router
- maxAgeLsa—Sets a trap to indicate that an LSA in this router LSDB has reached MaxAge
- ifStateChange—Sets a trap to indicate a state change on an OSPF interface
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line

#### Mode

Router Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out