# tcp resequence-buffers vr-maximum

#### Syntax

[ ip ] tcp resequence-buffers [ vrf vrfName ] vr-maximum vrMaxValue

no [ ip ] tcp resequence-buffers [ vrf vrfName ] vr-maximum

#### Release Information

Command introduced before JunosE Release 7.1.0.
ip keyword made optional in JunosE Release 7.2.0.

#### Description

Defines the maximum number of buffers that the current or specified virtual router can use. Specifying a value of zero (0) turns off the limit assignment. The no version reverts the virtual router maximum value to its default (100 buffers).

#### Options

- ip—Optional keyword for use with older scripts
- vrfName—Name of the VRF; string of 1–32 alphanumeric characters
- vrMaxValue—Virtual router maximum in the range 1–65535

#### Mode

Global Configuration