Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# timers

#### Syntax

timers update invalid holddown flush

no timers

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures RIP timers. The no version restores the default values.

#### Options

- update—Interval in seconds at which routing updates are sent; default value is 30
- invalid—Interval in seconds after which a route is declared invalid (null); default value is 180
- holddown—Interval in seconds during which routing information regarding better paths is disregarded by the router; default value is 120
- flush—Interval in seconds that must pass before a route is removed from the routing table; set this value greater than the invalid value; default value is 300

#### Mode

Address Family Configuration, Router Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out