Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# subscriber

#### Syntax

subscriber { bridgedEthernet | ip } { user | user-prefix } userName
domain domainName [ { password | password-prefix } password ]
[ no-authenticate ]

no subscriber { bridgedEthernet | ip }

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures a local subscriber (when one cannot be obtained externally, as in PPP) on the E Series router to support authentication and configuration from the RADIUS server. The no version negates the command.

#### Options

- bridgedEthernet—Specifies bridgedEthernet as the upper interface type
- ip—Specifies IP as the upper interface type
- user—Employs the username as specified
- user-prefix—Appends the interface physical location to the username
- userName—RADIUS username
- domainName—Domain name
- password—Employs the password as specified
- password-prefix—Appends the interface physical location to the password
- password—RADIUS password
- no-authenticate—Disables authentication

#### Mode

Interface Configuration, Subinterface Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out