# graceful-restart

#### Syntax

[ no ] graceful-restart

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures hitless restart capability for OSPFv2. If high availability is active, the OSPF instance can perform a hitless restart when switching or failing over to the secondary SRP module. The no version disables OSPF graceful restart capability on the router.

#### Mode

Router Configuration