Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Creating a Two-Rate Rate-Limit Profile

# peak-burst

#### Syntax

peak-burst size { millisecond milliseconds }

no peak-burst

#### Release Information

Command introduced before JunosE Release 7.1.0.
milliseconds variable added in JunosE Release 8.1.0.

#### Description

Sets the peak burst for a rate-limit profile. The no version restores the default value, 100 ms; if 100ms is less than 8K, then 8K (8192).

#### Options

- size—Size in bytes in the range 1–4294967295
- milliseconds—Milliseconds in the range 1–10000

#### Mode

Rate Limit Profile Configuration

## Related Documentation

- Creating a Two-Rate Rate-Limit Profile

#### Published: 2010-10-19

Help
|
My Account
|
Log Out