Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# vlan advisory-tx-speed

#### Syntax

vlan advisory-tx-speed speed

no vlan advisory-rx-speed

#### Release Information

Command introduced in JunosE Release 7.2.0.

#### Description

Sets an advisory connect (Tx) speed that the LAC sends in the Tx connect speed to the LNS. The no version restores the default behavior, in which the Tx speed is not sent to the LNS.

#### Options

- speed—Speed in the range 0–2147483647 kbps; 0 indicates no advisory speed setting

#### Mode

Profile Configuration, Subinterface Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out