Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# suspicious-control-flow-detection protocol backoff-time

#### Syntax

suspicious-control-flow-detection protocol protocolValue backoff-time backoffTimeValue

no suspicious-control-flow-detection protocol protocolValue backoff-time

#### Release Information

Command introduced in JunosE Release 7.3.0.

#### Description

Sets the backoff expiration time when the flow is no longer considered suspicious for a specific protocol. The no version restores the default value of 300 seconds for a protocol.

#### Options

- protocolValue—Name of the protocol
- backoffTimeValue—Period of time in seconds; 0 or a number in the range 10–1000; a value of zero means that a suspicious flow does not change to the nonsuspicious state because of a timeout; if the low threshold value is zero and the backoff time is zero, the flow is only considered no longer suspicious if the rate (in packets per second) goes to zero

#### Mode

Global Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out