Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# set ip next-hop

#### Syntax

set ip next-hop { ipAddress | interface interfaceType interfaceSpecifier |
peerAddress }

no set ip next-hop [ ipAddress | peerAddress]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Indicates where to send packets that pass a match clause of a route map for policy routing. The no version removes the set clause from a route map.

| Note: Beginning with JunosE Release 7.1.0, this command is not supported for route maps used by the table-map command.

#### Options

- ipAddress—IP address of next hop to which packets are sent; does not need to be an adjacent router
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- peerAddress—On outbound route maps, disables the next hop-calculation by setting the next hop to the IP address of the BGP speaker; on inbound route maps, overrides any third-party next-hop configuration by setting the next hop to the IP address of the peer

#### Mode

Route Map Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out