Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# redistribute isis

#### Syntax

[ no] redistribute isis from { level-1 into level-2 | level-2 into level-1 }
route-map mapTag

#### Release Information

Command introduced in JunosE Release 8.2.0.

#### Description

Redistributes IPv6 routes from one IS-IS routing level into the other. The no version ends the redistribution.

#### Options

- level-1—Specifies the redistribution of routes from or into IS-IS level 1
- level-2—Specifies the redistribution of routes from or into IS-IS level 2
- mapTag—String of up to 32 alphanumeric characters specifying the route map applied to all routes from the source protocol; if you do not specify a route map, all routes are redistributed

#### Mode

Address Family Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out