Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Chapter 17, Configuring Dynamic Interfaces
- ppp multilink multiclass fragmentation

# Configuring Fragmentation on Multiclass MLPPP Interfaces

You can configure fragmentation on a multiclass MLPPP interface with the same fragment size as that of the MLPPP interface.

Before you configure fragmentation on the multiclass MLPPP interface:

- Ensure that fragmentation is enabled on the MLPPP interface.

  See Configuring MLPPP Fragmentation and Reassembly in Chapter 8, Configuring Multilink PPP.

To configure fragmentation on a multiclass MLPPP interface:

- Specify the QoS traffic classes to be fragmented.

  - To configure fragmentation on multilink classes in a dynamic profile:

    host1(config-profile)#ppp multilink multiclass fragmentation best-effort voice otherData video

  - To configure fragmentation on multilink classes in a static MLPPP interface:

    host1(config-if)#ppp multilink multiclass fragmentation best-effort voice otherData video

  The order of the QoS traffic classes does not affect the execution of the command.

  | Note: You must include the best-effort traffic class in the ppp multilink multiclass fragmentation command, or the command fails.

## Related Documentation

- Chapter 17, Configuring Dynamic Interfaces
- ppp multilink multiclass fragmentation

#### Published: 2010-10-13

Help
|
My Account
|
Log Out