Country/Region

- United States
- ASEAN Region
- Australia
- 中国 - China
- France
- Deutschland - Germany
- India
- Italia - Italy
- 日本 - Japan
- 대한민국 - Korea
- Россия - Russia
- España - Spain
- 台灣 - Taiwan
- United Kingdom

Contact Us
|
Country/Region
United States

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# vlan auto-configure

#### Syntax

vlan auto-configure upperInterfaceType [ lockout-time { minTime maxTime |
none } ]

no vlan auto-configure upperInterfaceType [ lockout-time ]

#### Release Information

Command introduced in JunosE Release 7.1.0.
lockout-time keyword added in JunosE Release 7.3.0.

#### Description

Specifies the types of dynamic upper interface encapsulations that are accepted or detected by a dynamic VLAN subinterface. You can issue this command repeatedly in Profile Configuration mode to include autodetection of multiple upper interface encapsulation types within the base profile for a dynamic VLAN subinterface. The no version terminates detection of the specified encapsulation type.

#### Options

- upperInterfaceType—One of the following dynamic encapsulation types:
  - ip
  - pppoe
- minTime—Minimum lockout time in the range 1–86400 seconds (24 hours); default value is 1 second
- maxTime—Maximum lockout time in the range 1–86400 seconds (24 hours); default value is 1 second
- none—Disables lockout time for the specified dynamic encapsulation type

#### Mode

Profile Configuration

#### Published: 2010-10-19

Help
|
My Account
|
Log Out