# LM-10 ADV Line Module

> Module label | ES2 10G ADV LM
> Number of ports | Not applicable
> Software release | First supported: 10.1.0
> Description | 190 W maximum Acts as frame forwarding engines for the physical interfaces Processes up to 10 Gb of data traffic Pairs with ES2–S2 10GE PR IOA, ES2-S1 REDUND IOA, ES2–S3 GE-20 IOA, and ES2–S1 GE-8 IOA In an SRP-120 and SRP-320 configuration, it can be installed in any slot
> Type | TFA ASIC
> Capability | Supports a line rate of 128–byte frames on IOAs The 120–Gbps and 320–Gbps switch fabrics allocate 10 Gbps of overall bandwidth to each line module slot. See JunosE System Basics Configuration Guide, Chapter 6, Managing Modules for more information.
> Software features | Not applicable
> Line module compatibility | Not applicable
> SRP module compatibility | SRP-120 SRP-320
> Line module redundancy compatibility | Yes (Redundancy IOA must be installed in either slot 0 or slot 11) Can back up another ES2 10G ADV LM or ES2 10G LM Shared tunnel server on the ES2 10G ADV LM supports line module redundancy.
> Port redundancy support | Not applicable
> Cables and connectors | Not applicable
> LEDs | When lit, LED indicates: OK (green)—Self-test passed FAIL (red)—Failure detected ONLINE (green)—Online with no alarms or errors REDUN (green)—Redundant card available
> Alarms, errors, and events | See Monitoring Modules in JunosE System Basics Configuration Guide, Chapter 6, Managing Modules.