Log in
|
How to Buy
|
Contact Us
|
United States (Change)

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# path overhead c2

#### Syntax

For channelized OCx/STMx interfaces:

[ no ] path pathChannel overhead c2 byteValue

For unchannelized OCx/STMx interfaces:

[ no ] path overhead c2 byteValue

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Overrides the default value of the path signal label (C2) byte for SONET and SDH interfaces. The no version restores the default setting, which depends on the types of interface layers configured above the SONET/SDH interface.

#### Options

- pathChannel—Number, in the range 1–2147483648, that identifies the path on a channelized interface
- byteValue—Value for C2 byte; integer, in the range 0–255

#### Mode

Controller Configuration

#### Published: 2011-01-07

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice
Help
|
My Account
|
Log Out