Log in
|
How to Buy
|
Contact Us
|
United States (Change)

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Monitoring Forwarding and Drop Rates on the Egress Queue
- Troubleshooting Memory and Processor Use for Egress Queue Rate Statistics and Events

# show egress-queue rates

#### Syntax

show egress-queue rates [ color ] [ previous | current ] [ full | brief ]
{ interface interfaceType interfaceSpecifier |
l2tp session sessionName | tunnel-server interfaceType } [ atmVpi | s-vlanIdValue ]
[ explicit | summary ] [ traffic-class trafficClassName ]
[ rate-exceeding rateExceedingNumber { aggregate | committed | conformed |
exceeded | forwarded | minimum | maximum } ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
atmVpi and s-vlanIdValue variables added in JunosE Release 7.1.0.

#### Description

Displays statistics associated with egress queuing rates.

#### Options

- color—Displays drop rates by color without minimum and maximum rates, rather than as an aggregate of all colors
- previous—Displays rate statistics for the previous rate period; the default option
- current—Displays rate statistics for the current rate period
- full—Displays rate statistics for all queues
- brief—Displays rate statistics only for queues that have queue rate statistics enabled; the default option
- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- sessionName —Name of the L2TP session
- atmVpi—Virtual path identifier of this PVC; number in the range 0–255
- s-vlanIdValue—S-VLAN ID number in the range 0–4095
- explicit—Displays rate statistics for queues only on the specified interface and not queues stacked above the interface
- summary—Displays the sum of rates for the queues bound to interfaces that are stacked above the specified interface
- trafficClassName—Name of a traffic class for which egress queue rate statistics are displayed
- rateExceedingNumber—Bits per second in the range 1–1073741824
- aggregate—Displays queues in which the aggregate drop rate exceeds the rateExceedingNumber
- committed—Displays queues in which the committed drop rate exceeds the rateExceedingNumber
- conformed—Displays queues in which the conformed drop rate exceeds the rateExceedingNumber
- exceeded—Displays queues in which the exceeded drop rate exceeds the rateExceedingNumber
- forwarded—Displays queues in which the forwarding rate exceeds the rateExceedingNumber
- minimum—Displays queues in which the minimum queue rate exceeds the rateExceedingNumber
- maximum—Displays queues in which the maximum queue rate exceeds the rateExceedingNumber
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

## Related Documentation

- Monitoring Forwarding and Drop Rates on the Egress Queue
- Troubleshooting Memory and Processor Use for Egress Queue Rate Statistics and Events

#### Published: 2011-01-07

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice
Help
|
My Account
|
Log Out