Log in
|
How to Buy
|
Contact Us
|
United States (Change)

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# set dhcp relay max-client-packet-rate

#### Syntax

[ no ] set dhcp relay max-client-packet-rate [ packetsPerSecond ]

#### Release Information

Command introduced in JunosE Release 11.2.0.

#### Description

Configures DHCP relay to limit the maximum number of client packets that DHCP relay processes per second. The no version returns to the default, in which DHCP relay processes 4096 packets per second.

#### Options

- packetsPerSecond—Number of client packets that are processed per second in the range 0–4096.

#### Mode

Global Configuration

#### Published: 2011-01-07

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice
Help
|
My Account
|
Log Out