Log in
|
How to Buy
|
Contact Us
|
United States (Change)

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# ip vrrp accept-data

#### Syntax

[ no ] ip vrrp vrid accept-data

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Enables the backup router to process packets with an IP destination address equivalent to the virtual addresses while the backup router is in the master state. The router ignores this attribute when the VRRP entry uses a priority of 255. You must use the default state (disabled) to comply with RFC 3768. When disabled, the master router drops any packets with an IP destination address equivalent to the virtual address. The no version restores the default value, disabled.

| Note: When using this attribute and also restricting incoming packets to ICMP only, you must use policy filters to accept only ICMP packets with the virtual address as the destination address.

#### Options

- vrid—VRID identifier; a number in the range 1–255

#### Mode

Interface Configuration

#### Published: 2011-01-10

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice
Help
|
My Account
|
Log Out