### JunosE 12.0.0 Release Notes

> ### Errata

> This section identifies errors found in the JunosE documentation. These errors are corrected in subsequent releases of the affected documentation.

> - In the JunosE 8.2.x BGP and MPLS Configuration Guide, the following figures are missing in the HTML version:
> - L2VPN Components figure in the Overview section of the Configuring L2VPNs chapter
> - Topology for VPLS Configuration Example with LDP Signaling figure in the VPLS Configuration Example with LDP Signaling section of the Configuring VPLS chapter

> The omitted figures are included in the HTML version of the JunosE 9.0.x BGP and MPLS Configuration Guide in the following sections:

> - L2VPN Components figure in the L2VPN Components section of the L2VPNs Overview chapter
> - Topology for VPLS Configuration Example with LDP Signaling figure in the VPLS Configuration Example with LDP Signaling section of the Configuring VPLS chapter
> - The ERX7xx Models, ERX14xx Models, and the ERX310 Broadband Services Router section of JunosE System Basics Configuration Guide, Chapter 6, Managing Modules failed to mention that the ERX7xx models, ERX14xx models, and the ERX310 Broadband Services Router do not support hot-swap of the SRP IOA.

> See the JunosE 12.0.x System Basics Configuration Guide for updated information.

> - In the Configuring a Profile section in JunosE Link Layer Configuration Guide, Chapter 17, Configuring Dynamic Interfaces, the ppp authentication command section erroneously omits the following information from the list of guidelines:

> If the VR specified in a profile with the ipv6 virtual-router command differs from the VR provided by AAA, IPv6 uses the VR provided by AAA when the dynamic IPv6 upper-layer interface is created.

> - The Monitoring Redundancy in Installed Hardware section in JunosE Service Availability Configuration Guide, Chapter 2, Managing Module Redundancy fails to state the following additional information regarding the show environment all command that is used to display system environment information for an E320 router.

> You can use the show environment all command for ES2 4G line modules configured with Service IOAs on E120 and E320 routers to view information related to line module high availability configuration.

> The following example displays information about the slots in which primary and secondary line modules that are configured and activated for stateful line module switchover reside. The information that relates to stateful line module switchover is highlighted in bold and appears in the line after the line module redundancy detail.

> host1#show environment all
> chassis: 17 slot (id 0x3, rev. 0x0)
> fabric: 100 Gbps (rev. 1)
> fans: fanSubsystemOk
> nvs: ok (977MB flash disk, 29% full), matches running config
> power: A ok, B not present
> srp redundancy: mode is file-system-synchronization auto-sync
> enabled, switch-on-error enabled
> status unknown
> *** slots: cards missing or offline
> online: 0 6 13
> offline: 7
> empty: 1 2 3 4 5 11 12 14 15 16
> fabric slots: ok
> online: 6 7 8 9 10
> line redundancy: none
> line card HA:
> high availability is configured on slots:
> {0, 13}
> high availability state is active on slots:
> {0, 13}
> temperature: ok
> timing: primary
> primary: internal SC oscillator (ok)
> secondary: internal SC oscillator (ok)
> tertiary: internal SC oscillator (ok)
> auto-upgrade enabled
> fabric redundancy: ok
> *** system operational: no
> temperature temperature
> slot type (10C - 70C) status
> ---- ------------------ ----------- -----------
> 0 LM-4 42 normal
> 0/1 GE-4 IOA 23 normal
> 6 SRP-100 32 normal
> 6 SFM-100 32 normal
> 6/0 SRP IOA 25 normal
> 7 SFM-100 30 normal
> 8 SFM-100 23 normal
> 9 SFM-100 25 normal
> 10 SFM-100 24 normal
> 13 LM-4 24 normal
> 13/0 GE-4 IOA 23 normal
> fabric temperature ranges
> below -5C is too cold
> above 80C is too hot
> low temperature warning below 10C
> high temperature warning above 70C
> processor temperature ranges
> below -5C is too cold
> above 80C is too hot
> low temperature warning below 10C
> high temperature warning above 70C
> IOA temperature ranges
> below -5C is too cold
> above 80C is too hot
> low temperature warning below 10C
> high temperature warning above 70C

> The descriptions of the fields related to line module high availability are as follows:

> - line card HA—Configuration details for stateful line module switchover on E120 and E320 routers:
> - high availability is configured on slots—Slot numbers of the pairs of primary and secondary line modules configured on a single chassis for stateful switchover.
> - high availability state is active on slots—Slot numbers of the pairs of primary and secondary line modules activated for stateful switchover.
> - The Service Modules table in ERX Module Guide, Appendix A, Module Protocol Support incorrectly states that IPv6 Neighbor Discovery is not supported on the Service line module. In fact, IPv6 Neighbor Discovery is supported on ERX routers that contain a Service line module.

Copyright © 2011, Juniper Networks, Inc. Report An Error