Log in
|
How to Buy
|
Contact Us
|
United States (Change)

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# nas-port-type atm

#### Syntax

nas-port-type atm { adsl-cap | adsl-dmt | idsl | sdsl | xdsl | cable | wireless-80211 |
wireless-cdma | wireless-umts | wireless-1x-ev | wireless-other | iapp | value }

no nas-port-type atm

#### Release Information

Command introduced before Release 7.1.0.

#### Description

Specifies the RADIUS NAS-Port-Type attribute (61) used for ATM interfaces. The no version removes the NAS-Port-Type setting.

#### Options

- adsl-cap—Asymmetric DSL, Carrierless Amplitude Phase Modulation
- adsl-dmt—Asymmetric DSL, Discrete Multi-Tone
- idsl—ISDN DSL
- sdsl—Symmetric DSL
- xdsl—DSL of unknown type
- cable—Cable
- wireless-80211—Wireless 802.11
- wireless-cdma—Wireless code division multiple access (CDMA)
- wireless-umts—Wireless universal mobile telecommunications system (UMTS)
- wireless-1x-ev—Wireless 1xEV
- wireless-other—Wireless other
- iapp—Inter Access Point Protocol (IAPP)
- value—Number in the range 0–65535

#### Mode

AAA Profile Configuration

#### Published: 2011-01-07

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice
Help
|
My Account
|
Log Out