Log in
|
How to Buy
|
Contact Us
|
United States (Change)

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# path overhead j1

#### Syntax

For channelized OCx/STMx interfaces:

[ no ] path pathChannel overhead j1 { msg | exp-msg } [ message ]

For unchannelized OCx/STMx interfaces:

[ no ] path overhead j1 { msg | exp-msg } [ message ]

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies trace messages to check for connectivity between the router and the SONET/SDH device at the other end of the line. The no version restores the default situation, in which all characters of the trace message are zeros.

#### Options

- pathChannel—Number, in the range 1–2147483648, that identifies the path on a channelized interface
- msg—Specifies that the message is one that the router sends
- exp-msg—Specifies that the message is one that the router expects to receive
- message—Text of the message; the maximum is 15 characters for SDH mode and 62 characters for SONET mode

#### Mode

Controller Configuration

#### Published: 2011-01-07

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice
Help
|
My Account
|
Log Out