Log in
|
How to Buy
|
Contact Us
|
United States (Change)

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# threshold

#### Syntax

threshold { sd-ber | sf-ber } rate

no threshold { sd-ber | sf-ber }

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Sets the threshold values for bit error rates used in APS/MSP alarms. This command applies only to the protect interface, and not to the working interface. The no version restores the default value, 5 (for the sd-ber bit error rate) or 3 (for the sf-ber bit error rate), for the specified alarm.

#### Options

- sd-ber—Bit error rate that specifies signal degradation
- sf-ber—Bit error rate that specifies signal failure
- rate—Integer n with available values depending on the bit error rate type you specify; a value of n corresponds to a rate of 10-n (10e-n) errors per second
  - For sd-ber, an integer in the range 5–9; default value is 5
  - For sf-ber, an integer in the range 3–5; default value is 3

#### Mode

Controller Configuration

#### Published: 2011-01-07

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice
Help
|
My Account
|
Log Out