Log in
|
How to Buy
|
Contact Us
|
United States (Change)

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Monitoring the QoS Profiles Attached to an Interface
- Monitoring the QoS Scheduler Hierarchy
- Monitoring Shared Shapers
- controlled-interface-type
- instance-interface-type
- qos-interface-set
- qos-interface-superset
- qos-parameter
- qos-profile

# Creating a QoS Parameter on an Interface Superset or Interface Set

Tasks to create a QoS parameter on an interface superset or an interface set include:

## Configuring a QoS Parameter Definition for an Interface Superset or an Interface Set

You can configure a parameter definition to recognize an interface superset or an interface set as controlled-interface types and instance interface-types.

Controlled-interface types specify resources that the parameter instance can control. Instance-interface types are the interface types to which the QoS client can apply a parameter instance.

To specify an interface set or an interface superset in a QoS parameter definition:

1. Specify the QoS parameter definition.
   host1(config)#qos-parameter-define business
2. Configure the controlled-interface type and specify the interface set or the interface superset.
   host1(config-qos-parameter-define)#controlled-interface-type set host1(config-qos-parameter-define)#controlled-interface-type superset

   You can specify up to four controlled-interface types for each parameter definition.

3. Configure the instance-interface type and specify the interface set or the interface superset.
   host1(config-qos-parameter-define)#instance-interface-type set host1(config-qos-parameter-define)#instance-interface-type superset

   You can specify up to eight instance-interface types for each parameter definition.

## Creating a QoS Parameter Instance for an Interface Superset

To create a QoS parameter instance for an interface superset:

1. Specify the QoS interface superset.
   host1(config)#qos-interface-superset vlan-superset
2. Create the QoS parameter instance.
   host1(config-qos-interface-superset)#qos-parameter business-data
3. Attach the QoS profile.
   host1(config-qos-interface-superset)#qos-profile vlan

## Creating a QoS Parameter Instance for an Interface Set

To create a QoS parameter instance for an interface set:

1. Specify the QoS interface set.
   host1(config)#qos-interface-set vlan-set
2. Create the QoS parameter instance.
   host1(config-qos-interface-set)#qos-parameter business-data
3. Attach the QoS profile.
   host1(config-qos-interface-set)#qos-profile vlan

## Related Documentation

- Monitoring the QoS Profiles Attached to an Interface
- Monitoring the QoS Scheduler Hierarchy
- Monitoring Shared Shapers
- controlled-interface-type
- instance-interface-type
- qos-interface-set
- qos-interface-superset
- qos-parameter
- qos-profile

#### Published: 2010-12-15

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice
Help
|
My Account
|
Log Out