Log in
|
How to Buy
|
Contact Us
|
United States (Change)

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Stateful SRP Switchover Redundancy Modes
- Guidelines for Activating High Availability
- redundancy
- mode

# Activating High Availability

The switch route processor (SRP) module can operate in one of the two redundancy modes—file system synchronization and high availability. When you activate high availability, the router uses mirroring to keep the configuration and state of the standby SRP module coordinated with the configuration and state of the active SRP module.

To activate high availability:

1. From Global Configuration mode, launch Redundancy Configuration mode.
   host1(config)#redundancy
2. In Redundancy Configuration mode, specify high availability as the redundancy mode.
   host1(config-redundancy)#mode high-availability

## Related Documentation

- Stateful SRP Switchover Redundancy Modes
- Guidelines for Activating High Availability
- redundancy
- mode

#### Published: 2010-12-29

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice
Help
|
My Account
|
Log Out