Log in
|
How to Buy
|
Contact Us
|
United States (Change)

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Configuring Event Statistics
- show egress-queue events

# Monitoring Forwarding and Drop Events on the Egress Queue

#### Purpose

Display information about forwarding and drop event counts on the egress queue.

#### Action

To display events for a specific interface:

    host1# show egress-queue events interface gigabitEthernet 1/0
                                                committed  conformed  exceeded     rate
                            traffic  forwarded     drop       drop       drop     period
          interface          class     events     events     events     events     count
    ----------------------  -------  ---------  ---------  ---------  ---------  ---------
    ip GigabitEthernet1/0   tc1            132         0          0          0        132
                            tc2            132       132          0          0        132
                            tc3              6         0        132          0        132
                            tc4              0         0          0        132        132

To display events for an L2TP session:

    host1#show egress-queue events l2tp-session session1

To display events for a tunnel interface, specify the interface at the root of the scheduler hierarchy located on the tunnel-service interface or at the same hierarchy for LNS GRE tunnel traffic:

    host1#show egress-queue events tunnel-server 6/0

To display events for queues only on the specified interface and not stacked above the interface:

    host1#show egress-queue events gigabitEthernet 1/0 explicit

To display the sum of events for the queues bound to interfaces that are stacked above the specified interface:

    host1#show egress-queue events gigabitEthernet 1/0 summary

To display events for queues belonging to a specific traffic class:

    host1#show egress-queue events gigabitEthernet 1/0 traffic-class voice

To filter output based on the number of events that exceed the specified value.

    host1#show egress-queue events gigabitEthernet 1/0 event-exceeding committed
    host1#show egress-queue events gigabitEthernet 1/0 event-exceeding conformed
    host1#show egress-queue events gigabitEthernet 1/0 event-exceeding exceeded
    host1#show egress-queue events gigabitEthernet 1/0 event-exceeding forwarded

#### Meaning

Table 1 lists the show egress-queue events command output fields.

Table 1: show egress-queue events Output Fields

Field Name | Field Description
--- | ---
interface | Name of the interface
traffic class | Name of the traffic class
forwarded events | Number of forwarded rate events
committed drop events | Number of committed drop events
conformed drop events | Number of conformed drop events
exceeded drop events | Number of exceeded drop events
rate period count | Time frame during which events are counted (in seconds)

## Related Documentation

- Configuring Event Statistics
- show egress-queue events

#### Published: 2010-12-15

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice
Help
|
My Account
|
Log Out