Log in
|
How to Buy
|
Contact Us
|
United States (Change)

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- DHCP External Server Identification of Clients with Duplicate MAC Addresses Overview
- Configuring DHCP External Server to Uniquely Identify Clients with Duplicate MAC Addresses

# dhcp-external duplicate-mac-address

#### Syntax

[ no ] dhcp-external duplicate-mac-address

#### Release Information

Command introduced in JunosE Release 9.3.0.

#### Description

Configures the DHCP external server application to use a combination of the MAC address and the gateway IP address (giaddr) to uniquely identify DHCP clients attached to the router. This behavior is also referred to as duplicate MAC mode. The no version restores the default behavior, also known as unique MAC mode, which uses only the MAC address to uniquely identify DHCP clients.

#### Mode

Global Configuration

## Related Documentation

- DHCP External Server Identification of Clients with Duplicate MAC Addresses Overview
- Configuring DHCP External Server to Uniquely Identify Clients with Duplicate MAC Addresses

#### Published: 2011-01-10

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice
Help
|
My Account
|
Log Out