# pppoe auto-configure

#### Syntax

pppoe auto-configure [ lockout-time { minValue maxValue | none } ]

no pppoe auto-configure

#### Release Information

Command introduced before JunosE Release 7.1.0.
lockout-time keyword, minValue variable, maxValue variable, and none keyword added in JunosE Release 7.2.0.

#### Description

Configures the router to dynamically create PPPoE subinterfaces over static PPPoE major interfaces. Optionally, specifies the lockout time range for the PPPoE clients associated with the dynamic PPPoE subinterface column on the PPPoE major interface. The no version terminates dynamic creation of PPPoE subinterfaces on the static PPPoE major interface.

#### Options

- minValue—Minimum lockout time, in the range 1–86400 seconds (24 hours)
- maxValue—Maximum lockout time, in the range 1–86400 seconds (24 hours)
- none—Disables lockout for the PPPoE clients associated with the dynamic PPPoE subinterface column on the static PPPoE major interface; this is the default value

#### Mode

Interface Configuration, Subinterface Configuration