Log in
|
How to Buy
|
Contact Us
|
United States (Change)

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Configuring Shadow Nodes

# shadow-node

#### Syntax

[ no ] typeOfInterface shadow-node [ group trafficClassGroup | scheduler-profile
schedulerProfileName ]*

#### Release Information

Command introduced in JunosE Release 8.0.0.

#### Description

Specifies that a shadow node be configured for each interface of the given interface type. The no version removes this rule from the QoS profile.

#### Options

- typeOfInterface—Interface types for shadow nodes to be configured: atm, atm-vc, atm-vp, bridge, ethernet, fr-vc, ip, ip-tunnel, ipv6, l2tp-session, l2tp-tunnel, lsp, serial, server-port, svlan, vlan
- trafficClassGroup—Name of the traffic-class group
- schedulerProfileName—Name of the scheduler profile
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line

#### Mode

QoS Profile Configuration

## Related Documentation

- Configuring Shadow Nodes

#### Published: 2011-01-07

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice
Help
|
My Account
|
Log Out