Log in
|
How to Buy
|
Contact Us
|
United States (Change)

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Configuring 802.3ah OAM Link-Fault Management
- show ethernet oam lfm status

# Monitoring OAM Link-Fault Management Configuration for an Interface

#### Purpose

Display the current Ethernet OAM link-fault management configuration for a particular interface, such as the discovery mode of the interface, the interval at which OAM PDUs are transmitted to the remote peer, the number of OAM PDUs that can be missed from the remote peer before a link-fault event is generated, actions that are taken when the high threshold for an error is exceeded or when an OAM PDU from a remote peer signifies a fault condition, link monitoring attributes, and remote loopback settings.

#### Action

To display the runtime settings of link-monitoring and general OAM operations for a particular interface:

    host1#show ethernet oam lfm status GigabitEthernet 4/0
    GigabitEthernet 4/0
      Mode:                   Passive
      Transmit-interval:      1000 ms
      Loss-threshold:	        5 packets
      Event Action:           disable
      High Threshold Action:  disable
      Remote-loopback:        supported

    Frame-seconds Error Monitor
      Window:                 30 (100 millisecond units)
      Low threshold:          20 errored frames
      High threshold:         none

    Remote-loopback:
      Frames sent:            104437
      Bytes sent:             16167885

      Frames received:        104437
      Bytes received:	         16167885

#### Meaning

Table 1 lists the show ethernet oam lfm status command output fields.

Table 1: show ethernet oam lfm status Output Fields

Field Name | Field Description
--- | ---
Interface type/name interfaceSpecifier | Name and type of the Ethernet interface, in the interface specifier format, for which link-fault management packet details are displayed
Mode | Discovery mode of the interface: Active—The interface discovers and monitors the peer on the link if the peer also supports IEEE 802.3ah OAM functionality. An OAM entity in active mode initiates the discovery process by sending an Information OAM PDU to the multicast address of the slow protocol (0180.c200.0002) at a configured rate. The default discovery mode of the OAM client is active Passive—An OAM entity does not initiate the discovery process. You cannot perform link-fault management if you configure both the local client and the remote peer for passive mode operation
Transmit-interval | Number of milliseconds, after which Information OAM PDUs are sent from the local OAM entity to the remote peer to maintain the OAM association in an active state
Loss-threshold | Number of Information OAM PDUs that can be missed from the remote peer before a link fault event is triggered
Event Action | Action to be performed on an interface when an Information OAM PDU is received from the remote peer by the local OAM entity to signal a fault condition at the remote entity. Possible values are: disable—Sets the OAM functionality to unconditionally attempt to influence the operational state of the interface to down failover—On GE-2 and GE-HDE line modules that are paired with GE-2 SFP I/O modules with physical link redundancy, causes the transition of the link from active to redundant
High Threshold Action | Action that occurs when the high threshold for an error is exceeded: disable—Sets the OAM functionality to unconditionally attempt to influence the operational state of the interface to down. If the interface is a member link of a LAG bundle and at least one other viable link (redundant member or another active/up link) is present, OAM attempts to influence the operational state of the link to down. Otherwise, no action is taken failover—On GE-2 and GE-HDE line modules that are paired with GE-2 SFP I/O modules with physical link redundancy, causes the transition of the link from active to redundant
Remote-loopback | Indicates whether the local interface is enabled for remote loopback functionality and whether it can respond to remote loopback requests from peers: supported or unsupported. An OAM entity can put its remote peer into loopback mode using the Loopback control OAM PDU. In loopback mode, every frame received is transmitted back on the same port (except for OAM PDUs, which are needed to maintain the OAM session) to the local entity
Frame-seconds Error Monitor | Displays a detailed classification of frame seconds errors event TLVs since the OAM sublayer was reset
Window | Specified amount of time in milliseconds during which frame seconds error events are counted
Low threshold | Lowest value for frame second error events in number of frames, which when exceeded causes an Errored Frame Seconds Summary Event TLV to be sent to the peer
High threshold | Highest value for frame second error events in number of frames, which when exceeded causes an action to be triggered
Frame-errors Error Monitor | Displays a detailed classification of frame errors event TLVs since the OAM sublayer was reset
Window | Specified amount of time in hundred-millisecond units during which frame error events are counted
Low threshold | Lowest value for frame error events in number of frames, which when exceeded causes an Errored Frame Event TLV to be sent to the peer
High threshold | Highest value for frame error events in number of frames, which when exceeded causes an action to be triggered
Symbol-errors Error Monitor | Displays a detailed classification of symbol errors event TLVs since the OAM sublayer was reset
Window | Specified amount of time in seconds during which symbol error events are counted
Low threshold | Lowest value for frame second error events in number of error symbols, which when exceeded causes an Error Symbol Period TLV to be sent to the peer
High threshold | Highest value for symbol error events in number of error symbols, which when exceeded causes an action to be triggered
Remote-loopback | Displays details on the non-OAM PDUs that are sent and received when the interface is in remote loopback mode
Frames sent | Number of frames sent to the remote peer that are transmitted back or looped to the local interface
Bytes sent | Number of bytes sent to the remote peer that are transmitted back or looped to the local interface
Frames received | Number of frames received from the remote peer when the local entity is in loopback mode
Bytes received | Number of bytes received from the remote peer when the local entity is in loopback mode

## Related Documentation

- Configuring 802.3ah OAM Link-Fault Management
- show ethernet oam lfm status

#### Published: 2011-01-02

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice
Help
|
My Account
|
Log Out