Log in
|
How to Buy
|
Contact Us
|
United States (Change)

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# vlan advisory-rx-speed

#### Syntax

vlan advisory-rx-speed speed

no vlan advisory-rx-speed

#### Release Information

Command introduced in JunosE Release 7.2.0.

#### Description

Sets an advisory receive (Rx) speed that the LAC sends to the LNS. The no version restores the default behavior, in which the Rx speed is not sent to the LNS.

#### Options

- speed—Speed in the range 0–2147483647 kbps; 0 indicates no advisory speed setting

#### Mode

Profile Configuration, Subinterface Configuration

#### Published: 2011-01-07

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice
Help
|
My Account
|
Log Out