Log in
|
How to Buy
|
Contact Us
|
United States (Change)

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Guidelines for Managing Queue Thresholds
- Guidelines for Managing Buffers
- To identify the type of ASIC used by a line module, see the ERX Module Guide and the E120 and E320 Module Guide

# Memory Requirements for Queue and Buffers

JunosE Software uses 128-byte buffers.

The egress memory available for queues available depends on the ASIC and the line module. Table 1 lists the egress memory.

Table 1: Egress Memory and Region Size on ASIC Line Modules

ASIC | Line Module | Egress Memory (MB) | Region Size (MB)
--- | --- | --- | ---
EFA | All EFA line modules | 32 | 4
FFA | GE-2 and GE-HDE | 64 | 8
| OC48 | 128 | 16
ES2 4G LM | 128 | 16
TFA | ES2 10G LM | 96 | 12

## Related Documentation

- Guidelines for Managing Queue Thresholds
- Guidelines for Managing Buffers
- To identify the type of ASIC used by a line module, see the ERX Module Guide and the E120 and E320 Module Guide

#### Published: 2010-12-20

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice
Help
|
My Account
|
Log Out