Log in
|
How to Buy
|
Contact Us
|
United States (Change)

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Monitoring Shared Shapers

# show qos shared-shaper

#### Syntax

To display information about shared shapers for a specified interface:

show qos shared-shaper interface interfaceType interfaceSpecifier
[ atmVpi | s-vlanIdValue ] [ summary ] [ explicit ] [ brief | full ] [ filter ]

To display information about shared shapers on an L2TP session:

show qos shared-shaper lt2p session sessionName
[ summary ] [ explicit ] [ brief | full ] [ filter ]

To display information about shared shapers on a tunnel-service interface:

show qos shared-shaper tunnel-server interfaceType
[ summary ] [ explicit ] [ brief | full ] [ filter ]

To display information about shared shapers associated with an interface set:

show qos shared-shaper qos-interface-set interfaceSetName [ summary ] [ explicit ] [ brief | full ] [ filter ]

To display information about shared shapers associated with an interface superset:

show qos shared-shaper qos-interface-superset

interfaceSupersetName [ summary ] [ explicit ] [ brief | full ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
atmVpi and s-vlanIdValue variables added in JunosE Release 7.1.0.

qos-interface-set keyword and interfaceSetName variable added in JunosE Release 9.2.0.

qos-interface-superset keyword and interfaceSupersetName variable added in JunosE Release 9.2.0.

#### Description

Displays information about shared shapers for an interface, L2TP session, or tunnel-service interface.

#### Options

- interfaceType—Interface type; see Interface Types and Specifiers
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- atmVpi—Virtual path identifier of this PVC; number in the range 0–255
- s-vlanIdValue—S-VLAN ID number in the range 0–4095
- sessionName —Name of the L2TP session
- interfaceSetName—Name of the QoS interface set associated with the shared shaper
- interfaceSuperSetName—Name of the QoS interface superset associated with the shared shaper
- summary—Displays summary of shared shapers stacked above the specified interface
- explicit—Displays shared shapers for the specified interface rather than those stacked above the interface
- brief—Displays information in condensed format
- full—Displays information in expanded format
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

## Related Documentation

- Monitoring Shared Shapers

#### Published: 2011-01-07

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice
Help
|
My Account
|
Log Out