Log in
|
How to Buy
|
Contact Us
|
United States (Change)

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- See Monitoring BGP-Related Settings for L2VPNs in JunosE BGP and MPLS Configuration Guide

# show ip bgp filter-list

#### Syntax

show ip bgp [ ipv4 unicast | ipv4 multicast | vpnv4 all | vpnv4 vrf vrfName |
l2vpn all | l2vpn vpls vplsName | l2vpn vpws vpwsName | route-target signaling ]
filter-list asPathAccessListName [ fields fieldOptions ] [ filter ]

#### Release Information

Command introduced before JunosE Release 7.1.0.
l2vpn and all keywords added in JunosE Release 7.1.0.
vpls keyword and vplsName variable added in JunosE Release 7.1.0.
vpws keyword and vpwsName variable added in JunosE Release 8.1.0.
route-target signaling keywords added in JunosE Release 8.2.0.

#### Description

Displays all routes whose AS path matches the specified AS path access list.

#### Options

- ipv4 unicast—Specifies the IPv4 unicast address family and routing table; the default option
- ipv4 multicast—Specifies the IPv4 multicast address family and routing table
- vpnv4 all—Specifies the IPv4 VPN address family and all IPv4 VPN routing and forwarding instances
- vpvn4 vrf vrfName—Specifies the IPv4 VPN address family and only the IPv4 VPN routing and forwarding instance with the name vrfName
- l2vpn all—Specifies all VPLS and VPWS instances in the L2VPN address family
- l2vpn vpls vplsName—Specifies the VPLS instance with the name vplsName
- l2vpn vpws vpwsName—Specifies the VPWS instance with the name vpwsName
- route-target signaling—Displays information for only the route-target address family
- asPathAccessListName—Name of AS path access list to filter routes; displays only routes that have AS paths matching the specified list
- fields—Displays only the specified fields; the display order of the fields is hard-coded and not affected by the order in which you enter them
- fieldOptions—Fields to be displayed, in the format
  all | [ afi | aggregator | as-path | atomic-aggregate | best | clusters | communities | extended-communities | imported | intro | in-label | loc-pref | med | next-hop | next-hop-cost | origin | originator-id | out-label | peer | peer-type | rd | safi | stale | unknown-types | weight ]*
  - all—All available information; not recommended, because this information for each network does not fit on a single line and is difficult to read
  - afi—Address family identifier
  - aggregator—AS number and IP address of aggregator
  - as-path—AS path through which this route bas been advertised
  - atomic-aggregate—Whether the atomic aggregate attribute is present
  - best—Whether this is the best route for the prefix
  - clusters—List of cluster IDs through which the route has been advertised
  - communities—Community number associated with the route
  - extended-communities—Extended community
  - imported—Whether the route was imported
  - intro—Introductory information about the state of various BGP attributes; this information is displayed only if you specify this keyword
  - in-label—MPLS label for the route; the label received with incoming MPLS frames; typically, but not always, this is the label advertised to MP-BGP peers
  - loc-pref—Local preference for the route
  - med—Multiexit discriminator for the route
  - next-hop—IP address of the next router that is used when forwarding a packet to the destination network
  - next-hop-cost—Whether the indirect next hop of the route is unreachable, if not, displays IGP cost to the indirect next hop
  - origin—Origin of the route
  - originator-id—Router ID of the router in the local AS that originated the route
  - out-label—MPLS label for the route; the label sent with outgoing MPLS frames; also the label received from MP-BGP peer; typically, but not always, this is the label received from MP-BGP peers
  - peer—IP address of BGP peer from which route was learned
  - peer-type—Type of BGP peer: internal, external, or confederation
  - rd—Route distinguisher
  - safi—Subsequent address family identifier
  - stale—Route that has gone stale due to peer restart
  - unknown-types—Attribute codes for unknown path attributes
  - weight—Weight of the route
  - *—Indicates that one or more parameters can be repeated multiple times in a list in the command line
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec

## Related Documentation

- See Monitoring BGP-Related Settings for L2VPNs in JunosE BGP and MPLS Configuration Guide

#### Published: 2011-01-07

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice
Help
|
My Account
|
Log Out