Log in
|
How to Buy
|
Contact Us
|
United States (Change)

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# neighbor site-of-origin

#### Syntax

neighbor { ipAddress | ipv6Address | peerGroupName } site-of-origin siteOfOrigin

no neighbor { ipAddress | ipv6Address | peerGroupName } site-of-origin

#### Release Information

Command introduced before JunosE Release 7.1.0.
ipv6Address variable added in JunosE Release 8.0.0.

#### Description

Specifies a site of origin that is added to the extended communities list in each route received from the specified peer, unless the extended communities list already includes a site of origin. When routes are advertised to the peer, routes whose extended communities list contain this site of origin are filtered out and not advertised to the peer. After you issue this command, the site of origin is applied to all routes that are received or advertised. The session is not bounced.

The no version removes the site of origin for the peer.

| Note: To apply the new policy to routes that are already present in the BGP routing table, you must use the clear ip bgp command to perform a soft clear or hard clear of the current BGP session.

#### Options

- ipAddress—IP address of BGP neighbor
- ipv6Address—IPv6 address of BGP neighbor
- peerGroupName—Name of a BGP peer group. If you specify a BGP peer group by using the peerGroupName argument, all the members of the peer group inherit the characteristic configured with this command. You cannot override the characteristic for a specific member of the peer group.
- siteOfOrigin—Designator for the site of origin; in the format AA:NN, where any of the following is true:
  - AA—AS number in the range 0–65535 and NN is an integer in the range 0–4294967295; for example, 320:72358
  - AA—AS number in the range 0–4294967295 and NN is an integer in the range 0–65535; for example, 84511:45
  - AA—Dotted decimal IP address and NN is an integer in the range 0–65535; for example, 10.10.21.5:1256

#### Mode

Address Family Configuration, Router Configuration

#### Published: 2011-01-07

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice
Help
|
My Account
|
Log Out