# net

#### Syntax

[ no ] net networkEntityTitle

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Configures an IS-IS network entity title for the specified routing process. The no version removes a specific NET. You must specify a NET. You can add multiple manual area IDs by adding multiple NETs with the same system ID. The last NET cannot be removed.

#### Options

- networkEntityTitle—NET that specifies the area ID and the system ID for an IS-IS routing process; can be either an address or a name; in the form of: areaID.systemID.nSelector
  For example:
  - areaID—All bytes in front of the system ID; the number of bytes can vary from 1–13 bytes
  - systemID—Always 6 bytes and cannot vary
  - nSelector—Last byte; always 0

#### Mode

Router Configuration