# shadow-node

#### Syntax

[ no ] typeOfInterface shadow-node [ group trafficClassGroup | scheduler-profile
schedulerProfileName ]*

#### Release Information

Command introduced in JunosE Release 8.0.0.

#### Description

Specifies that a shadow node be configured for each interface of the given interface type. The no version removes this rule from the QoS profile.

#### Options

- typeOfInterface—Interface types for shadow nodes to be configured: atm, atm-vc, atm-vp, bridge, ethernet, fr-vc, ip, ip-tunnel, ipv6, l2tp-session, l2tp-tunnel, lsp, serial, server-port, svlan, vlan
- trafficClassGroup—Name of the traffic-class group
- schedulerProfileName—Name of the scheduler profile
- *—Indicates that one or more parameters can be repeated multiple times in a list in the command line

#### Mode

QoS Profile Configuration

#### Related Documentation

- Configuring Shadow Nodes