Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Rate and give feedback: Feedback Received. Thank You!
Rate and give feedback:
This document helped resolve my issue. Yes No

Additional Comments

800 characters remaining

May we contact you if necessary?

Name:
E-mail:

## Related Documentation

- QoS for 802.3ad Link Aggregation Interfaces Overview
- qos-port-type-profile

# Enabling Default Subscriber Load Balancing for 802.3ad Link Aggregation Groups

The factory default contents of the lag-default QoS profile include an Ethernet queue and the best-effort traffic class.

When you use the lag-default QoS profile, the system automatically sends traffic to the Ethernet queue and uses hash load balancing for the Ethernet queues.

To enable subscriber load balancing as the default behavior for all LAGs, issue the following command:

host1(config)#qos-port-type-profile lag qos-profile ethernet-default

## Related Documentation

- QoS for 802.3ad Link Aggregation Interfaces Overview
- qos-port-type-profile

#### Published: 2011-03-21

Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out