# ip igmp-proxy unsolicited-report-interval

#### Syntax

ip igmp-proxy unsolicited-report-interval tenths-of-a-second

no ip igmp-proxy unsolicited-report-interval

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies how often the upstream interface should transmit unsolicited reports. This command has no effect on interfaces other than the upstream value. The no version transmits unsolicited reports using the default value, 400 tenths of a second.

| Note: Issue this command only on the upstream interface. Otherwise, this command will have no effect.

#### Options

- tenths-of-a-second—Time interval at which the interface transmits unsolicited reports

#### Mode

Interface Configuration