# show pppoe interface lockout-time

#### Syntax

show pppoe interface [ interfaceType interfaceSpecifier ] lockout-time [ filter ]

#### Release Information

Command introduced in JunosE Release 7.2.0.

#### Description

In configurations with dynamic PPPoE subinterfaces over static PPPoE major interfaces, displays detailed information about the current encapsulation type lockout condition for each PPPoE client associated with the dynamic PPPoE subinterface column. The output of this command displays multiple entries for the same MAC Address, one for each interworking function (IWF) PPPoE session, if multiple IWF sessions contain the same MAC address.

#### Options

- interfaceType—One of the following interface types listed in Interface Types and Specifiers:
  - atm
  - fastEthernet
  - gigabitEthernet
  - lag
  - serial—PPPoE is not currently supported on serial interfaces
  - tenGigabitEthernet
- interfaceSpecifier—Particular interface; format varies according to interface type; see Interface Types and Specifiers
- filter—See Filtering show Commands

#### Mode

Privileged Exec, User Exec