# Monitoring BGP Routes with Nonnatural Network Masks

#### Purpose

Display information about routes that have nonnatural network masks. Report whether the indirect next hop of a route is unreachable; if not, display the IGP cost to the indirect next hop.

#### Action

To display information about routes that have nonnatural network masks:

    host1#show ip bgp cidr-only

    Local BGP identifier 111.111.111.111, local AS 444
      0 routes (0 bytes used), 0 distinct destinations (0 bytes used)
      0 routes selected for route table installation
      0 path attribute entries (0 bytes used)

    Status codes: > best, * invalid, s suppressed, d dampened, r rejected

      Prefix         Peer       Next-hop    MED LocPrf  Weight  Origin
      33.0.0.0/24   5.72.1.1   5.72.1.1     1           0       inc.
    > 44.44.0.0/24  0.0.0.0    192.168.1.1  1           32768   inc.

#### Meaning

Table 28 lists the show ip bgp cidr-only command output fields.

Table 28: show ip bgp cidr-only Output Fields

Field Name | Field Description
--- | ---
Local BGP identifier | BGP router ID of the local router
local AS | Local autonomous system number
routes | Total number of routes stored in the BGP routing table and amount of memory consumed by routes. If several peers have advertised a route to the same prefix, all routes are included in this count.
distinct destinations | Number of routes to unique prefixes stored in the BGP routing table. If several peers have advertised a route to the same prefix, only the best route is included in this count.
routes selected for route table installation | Number of routes in the BGP routing table that have been inserted into the IP routing table
path attribute entries | Number of distinct path attributes stored in BGP's internal path attributes table. If BGP receives two routes for different prefixes but with identical path attributes, BGP will create only one entry in its internal path attribute table and share it between the two routes to conserve memory.
Prefix | Prefix for the routing table entry
Peer | IP address of BGP peer
Next hop IP address | IP address of the next hop
MED | Multiexit discriminator for the route
LocPrf | Local preference for the route
Weight | Assigned path weight
Origin | Origin of the route

#### Related Documentation

- show ip bgp cidr-only