# Configuring BFD

You configure BFD on routing protocols that use BFD for fast failure detection. BFD does not require any stand-alone configuration; it works in conjunction with the application that it is supporting. Applications on which you configure BFD pass configuration information to BFD when they need fast failure detection.

BFD works with a wide variety of routing protocols. The JunosE Software currently supports only a few of these protocols. All BFD supported clients provide the ability to configure session parameters for each interface. Refer to the following table for added configuration information:

Configuration Topic | See
--- | ---
EBGP | Configuring BGP Routing in JunosE BGP and MPLS Configuration Guide
IPv4 static routes | Configuring IP in JunosE IP, IPv6, and IGP Configuration Guide
IS-IS | Configuring IS-IS in JunosE IP, IPv6, and IGP Configuration Guide
OSPF | Configuring OSPF in JunosE IP, IPv6, and IGP Configuration Guide
OSPFv3 | Configuring OSPF in JunosE IP, IPv6, and IGP Configuration Guide
PIM | Configuring PIM for IPv4 Multicast in JunosE IP, IPv6, and IGP Configuration Guide and Configuring PIM for IPv6 Multicast in JunosE Multicast Routing Configuration Guide
RIP | Configuring RIP in JunosE IP, IPv6, and IGP Configuration Guide
RSVP-TE | Configuring MPLS in JunosE BGP and MPLS Configuration Guide