# Monitoring Configuration Information for AAA Local Authentication

#### Purpose

Display the configuration information for AAA local authentication. You can display information for the following keywords:

- - databases—Local user databases configured on the router
  - users—Users configured in the local user databases
  - virtual-router—Local user database selected by the specified virtual router for local authentication
- For additional information about the show configuration command, see JunosE System Basics Configuration Guide.

#### Action

To display the configuration information for AAA local authentication:

    host1#show configuration category aaa local-authentication databases
    ! Configuration script being generated on TUE NOV 09 2004 12:50:18 UTC
    ! Juniper Edge Routing Switch ERX-1400
    ! Version: 6.1.0 (November 8, 2004  18:31)
    ! Copyright (c) 1999-2004 Juniper Networks, Inc.  All rights reserved.
    !
    ! Commands displayed are limited to those available at privilege level 15
    !
    ! NOTE:  This script represents only a subset of the full system configuration.
    ! The category displayed is: aaa local-authentication databases
    !
    hostname host1
    aaa new-model
    aaa local database default
    aaa local database svaleLdb10

#### Meaning

Table 22 lists the show configuration category aaa local-authentication command output fields.

Table 22: show configuration category aaa local-authentication Output Fields

Field Name | Field Description
--- | ---
aaa local database | Name of the local user database; the name default specifies the default local user database
aaa local select database | Local user database that the virtual router uses for local authentication
aaa local username | Unique user entry in the local user database
database | Name of the local user database for the specified username
hostname | Name of the host router
ip-address | IP address parameter for the user entry
ip-address-pool | IP address pool parameter for the user entry
operational virtual-router | Virtual router parameter for the user entry
password | Password used to authenticate the subscriber
secret | Secret used to authenticate the subscriber
virtual-router | Name of virtual router

#### Related Documentation

- show configuration category aaa local-authentication