# ip igmp-proxy V1-router-present-time

#### Syntax

ip igmp-proxy V1-router-present-time seconds

no ip igmp-proxy V1-router-present-time

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies how long the router assumes that there is an IGMPv1 querier router on the subnet after the router receives an IGMP V1 query on this interface. The no version restores the default value, 10 seconds.

#### Options

- seconds—Time for which the router assumes that there is an IGMPv1 querier router on the subnet after the router receives an IGMP V1 query on this interface

#### Mode

Interface Configuration