# ipv6 ospf retransmit-interval

#### Syntax

ipv6 ospf [ processId ] retransmit-interval retransInterval

no ipv6 ospf [ processId ] retransmit-interval

#### Release Information

Command introduced before JunosE Release 7.1.0.

#### Description

Specifies the time between LSA retransmissions for the interface when an acknowledgment for the LSA is not received. The no version restores the default value.

#### Options

- processId—Integer in the range 1–65535
- retransInterval—Number in the range 0–3600 seconds; default value is 5 seconds

#### Mode

Interface Configuration, Subinterface Configuration